ldns-update(1)              General Commands Manual             ldns-update(1)



NAME
       ldns-update - send a dynamic update packet

SYNOPSIS
       ldns-update name [ zone ] [ ip ] [ tsig_name tsig_alg tsig_hmac ]


DESCRIPTION
       ldns-update is used to send a dynamic update packet.


OPTIONS
       name   The domainname to associate with the given ip address.


       zone   When  given uses this zone instead of trying to find and process
              domain's SOA record.


       ip     Send the update to this IP address.  Or, when the  literal  text
              none is given, remove any previous addresses.


       tsig_name tsig_alg tsig_hmac
              Use TSIG (rfc2845) to authenticate.


EXAMPLE
       ldns-update my.example.org 1.2.3.4


AUTHOR
       Written  by  Jakob Schlyter and Hkan Olsson, as an addition to the ldns
       library from NLnet Labs.


REPORTING BUGS
       Report bugs to <ldns-team@nlnetlabs.nl>.


COPYRIGHT
       Copyright (C) 2005 NLnet Labs. This is free software. There is NO  war-
       ranty;  not  even  for MERCHANTABILITY or FITNESS FOR A PARTICULAR PUR-
       POSE.



                                  30 May 2005                   ldns-update(1)
