ldns(3)                    Library Functions Manual                    ldns(3)



NAME
       ldns_buffer2pkt_wire - convert buffer/wire format to ldns_pkt


SYNOPSIS
       #include <stdint.h>
       #include <stdbool.h>

       #include <ldns/ldns.h>

       ldns_status ldns_buffer2pkt_wire(ldns_pkt **packet, const ldns_buffer
       *buffer);

DESCRIPTION
       ldns_buffer2pkt_wire() converts the data in the ldns_buffer (in wire
              format) to a DNS packet.  This function will initialize and
              allocate memory space for the packet structure.

              packet: pointer to the structure to hold the packet
              buffer: the buffer with the data
              Returns LDNS_STATUS_OK if everything succeeds, error otherwise

AUTHOR
       The ldns team at NLnet Labs.


REPORTING BUGS
       Please report bugs to ldns-team@nlnetlabs.nl or in our bugzilla at
       http://www.nlnetlabs.nl/bugs/index.html


COPYRIGHT
       Copyright (c) 2004 - 2006 NLnet Labs.

       Licensed under the BSD License. There is NO warranty; not even for MER-
       CHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.

SEE ALSO
       perldoc Net::DNS, RFC1034, RFC1035, RFC4033, RFC4034 and RFC4035.

REMARKS
       This manpage was automatically generated from the ldns source code.



                                  30 May 2006                          ldns(3)
